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LIST OF MATERIALS
NO. NO.
P/N DESCRIPTION EQ'D PIN DE T EQ'D
1 Side Rail 2 19 Metal Seat, Covered 1
2 Cross Bar 1 20 Floor Pan 1
3 Front Axle Bar 1 21 Motor Mount 1
4 Rear Axle Bar 1 (Plate 1/4" x 8-1/2" x 9)
5 Rear Axle 2 22  Front Wheel,Bearing 2
6 Steering Shaft 1 Mounted (4.10-3.50 x 5 tire)
7 Steering Wheel 1 23  Automatic Clutch 1
8 Cowling Collar 1 24  Rear Wheel with Brake X
(1/2" 1D Tube x 3") & Sprocket (4.10-3.50 x 5 tire)
8A Steering Shaft Plate 1 25 Rear Wheel with Brake o
9 Tie Rod with Clevis 2 (4.10-3.50 x 5 tire)
10  Right-Hand Axle Assy. 1 26  Driving Chain 1
11 Left-Hand Axle Assy. 1 27 Bolt (1/2"-13x4-1/2") 2
12  Cowling 1 For Front Axle Assy.
13  Brake Shaft 1 28 Bolt (3/8"-16x1") 1
14  Brake Lever 2 For Steering Shaft
15 Brake Linkage 2 29  Cotter Pins (1/8") 4
16  Brake and Gas Rod 2 For Brake & Gas Rods
17  Left Foot Pedal 1 30 Bolt(5/16"-18x1-1/4") 4
18  Right Foot Pedal 1 For Pedals & Tie Rods

INSTRUCTIONS FOR ASSEMBLY:

* NOTE: For twin motor drive, order two No. 24 wheels and cancel the No. 25 wheel.

First: Drill two 5/8" diameter holes in each end of the rear axle bar (No. 4) and weld the rear axles (No. 5) into place. Now
make a wooden fixture to hold Parts 1, 2, 3, and 4 together for welding. To line these parts up properly, first slide the
brakfe shaft (No. 13) through the 1/2" collars on the side rails (No. 1). Tighten all pieces to the wooden frame with clamps
or wire and weld where needed. Do NOT weld the brake shaft (No. 13)! Next, attach the front axle assemblies (Nos. 10 &
11) to the front axle bar (No. 3) using 1/2" - 13 bolts, and put on wheels. Slide the brake lever (No. 14) onto the brake
shaft (No. 13) and slip 5/8" collars on each rear axle shaft (No. 5), and bolt on the rear wheels. Attach the brake and gas
rod (No. 16) to the pedal with the cotter pin (No. 29). Then slide the rod through the brake lever (No. 14). Slide the brake
linkage (No. 15) on the rod and clamp the lever and the linkage together for later use. Repeat for the other side. Next
weld the floor pan (No. 20) in place. Weld the cowling (No. 12) with the collar (No. 8) to the cross bar (No. 2) at 35 '
degrees. Then slide the steering shaft (No. 6) through the collar into place. Bolt on the steering wheel (No. 7), and weld
the seat (No. 19) in place. Now attach the tie rods (No. 9) to the axle assemblies and the steering shaft using bolts.

Adjust as needed. Affix the motor mount (No. 21) and adjust the driving chain (No. 26). Once all final adjustments are
made and the brake lever (No. 14) and the brake linkage (No. 15) are clamped at the proper angle, weld together.

Now you're ready to go! M
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"LIL" INDIAN GO-KART

We do not sell completely assembled Go-Karts. We only sell individual parts which allows you to
custom build your own Go-Kart. You can choose the size and type of tires, size of wheels (5" or
6"), and size of drive sprocket. Buy only the parts you need to complete your Go-Kart. This is
an excellent project for father and son or daughter to get together and build. A good way to
teach them about the basics of mechanical assembly and proper maintenance.

* Live axle (drives both wheels) ’ * Hi speed precision wheel bearings

* 58" or 6" Aluminum wheels * Rubber insulated, bolt in floor pan (no welds to break)

* Heavy duty fiberglass seat * Heavy gauge (1/8" wall tubing) precision jig welded frame
* Wide wheel stance for more stability * Motor mount will accommodate most lawnmower style engines
* Akerman steering for positive turning * Caster and camber automotive type steering

* Tecumseh overhead valve 5 HP engine * Dropped front axle

* Tecumseh flat head 3 HP engine * Low roll center, track tested frame design

* Automatic centrifugal clutch * Frame overall length - 57"

* Kill switch on steering wheel *-Frame wheelbase - 44"

* Epoxy powder coated, baked on paint - black * Frame width - 15 1/2"

* Racing style brake and throttle pedals * Front axle width - 29 1/2"

* Steering Wheel (Chrome plated steel, soft plastic grip)  * Optional front and rear bumper

* Spot disc brake on rear axle * Optional side rails supports for seat

* Easy to replace, split sprocket * Can be shipped UPS

* Choice of sprocket size

To purchase all the parts neccessary to build a complete "LIL" INDIAN Go-Kart
order the following parts and parts packages.

PART NO. RETAIL
31006 Frame parts package B $319.95

31007 Rear axle parts package $149.95

31008 Power parts package, 5 HP $299.95

31009 Power parts package, 3 HP $254.95

97031 Brake control parts package $19.95

97032 Throttle control parts package $31.95

64021 (2),1117A (2) Front and rear wheels, 6" $135.80
1720020 (2) Front wheel bearing bushings for 6" wheels $5.00
10-064 (2), 10-069 (2), 08-354 (4)  Tires and tubes $117.60
2672X Split Sprocket, Choose number of teeth $24.50

All parts needed to build a complete 5 HP Go-Kart with 6" wheels $1104.85

All parts needed to build a complete 3 HP Go-Kart with 6" wheels $1059.65
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COMPLETE KART KITS�
�
Description�
Part No.�
�
Kart Kit with 5" Nylon Wheels�
� HYPERLINK "javascript:void(0)" �3557�  $605.95  + Shipping�
�
Kart Kit with 5" Aluminum Wheels�
� HYPERLINK "javascript:void(0)" �3551�   $615.95  + Shipping�
�
Kart Kit with 6" Aluminum Wheels�
� HYPERLINK "javascript:void(0)" �3552�   $709.95  +  Shipping�
�






Przyojski Motor Co. Kart Kits are compiled from quality components.�These parts, sub-assemblies and hardware offer a Kit designed to provide everything�necessary to assemble a Go-Kart - with the assurance that the parts fit, the hard-�ware is the proper size and quantity, and the weldments and sub-assemblies conform to �corporate standards of form, fit and function. Assembly instructions and parts lists for�each kit are included. We do not supply engines and therefore we do not preselect a �clutch. We do, however, carry an array of suitable 4-cycle clutches.











